# Install

This instruction was written on the assumption than CUPS is installed correctly.
To install these files, you must log in as "root" user. Or you must execute "su" to become a "root".

1. Copy the
2. Restart CUPS to recognize files.
   Execute the following command.

   /etc/rc.d/init.d/cups restart

3. Start a browser in your computer, and access to administration page.
   The "root"'s password is required from now, but you must not be a root user.
   - If you are using the computer to install files, click here to open the administration page.
   - If you are accessing another computer, access to http://xxx.xxx.xxx.xxx:631/
     In this case, assign xxx.xxx.xxx.xxx as name or an IP address of the computer to install.
     For example :
     http://192.168.0.1:631/
     or
     http://cups-pc.localnet.com:631/
   Right screen will be displayed on your browser, if you could access correctly (Click right images to Zoom). Click the image written "Manage Printer".
4. Right screen will be displayed on your browser.
   Click the image with "Add Printer" on your browser.
   If some other printers are already installed, informations about them are displayed. (If so, refer to the screen when intall is finished.)
5. Next, the browser requests user name and password like left screen.
   You must type "root" as user name, and password for root into this dialog box.
   Go to TOP
6. If your computer accepts user name and password, the browser displays a screen to input Printer Name, Printer Location, and Description.
   At this screen, you must type the Printer Name. It is used to identify the printer from all printers installed and it must be unique if any other printers are installed. (In the right sample screen, "CBM1000" is used as printer name.) If some spaces (" ") is included in the printer name, it will be complicated when you use lpoption command (or else) to indicate this printer.
   Location and Description are optional. You don't have to type any data.
   Click "Next" if you filled each data.
7. The browser displays rigth screen, if filled data are accepted.
   From the "Device" list, choose a port which the printer is connected, and click "Next".
8. Next, the browser shows a list of manufacturers.
   This ist of manufacuturers depends on the distribution of linux or printers already installed.
   Choose "CITIZEN" and click "Next".
   Go to TOP
9. Next, browser shows a list of models.
   If PPD files of both CBM1000 and CD-S500 are copied to the specified directory (described above), the list of models is displayed like right sample image.
   Choose a model to be installed, and click "Next"
10. If right screen would be displayed, installation is completed. Click "Printer" in the menu bar displayed in upper area.
11. Check that the infomation about installed printer is displayed.
    The right image is a example when CBM1000 was install as "CBM1000".
    After the printer is added, set it up (paper size , etc). And set this as a default printer, if it is needed.